I have configured VLAN segmentation by creating VLANs on the switch, assigning switch ports to the appropriate VLANs, setting IP addresses on the corresponding interfaces, and configuring trunk links between switches and the router. As shown in the topology, the setup is functioning correctly and devices within the same VLAN can communicate as expected.







